<?xml version="1.0"?>

<PropertyList>

  <!-- Specific keys -->

  <key>
    <name>=</name>
    <desc>Options menu</desc>
  </key>
  <key>
    <name>Shift+C</name>
    <desc>Toggle auto-coordination</desc>
  </key>
  <key>
    <name>D</name>
    <desc>Crew door view</desc>
  </key>
  <key>
    <name>Ctrl+D</name>
    <desc>Open/Close crew door</desc>
  </key>
  <key>
    <name>E</name>
    <desc>Engineer view</desc>
  </key>
  <key>
    <name>F, Shift+F</name>
    <desc>Open, close cowl flaps one step</desc>
  </key>
  <key>
    <name>J</name>
    <desc>Jump seat view</desc>
  </key>
  <key>
    <name>K</name>
    <desc>Cockpit observer view</desc>
  </key>
  <key>
    <name>L</name>
    <desc>Copilot view</desc>
  </key>
  <key>
    <name>Ctrl+L</name>
    <desc>Unlock/Lock Prop Reversing</desc>
  </key>
  <key>
    <name>Alt+L</name>
    <desc>Run After Landing Checklist</desc>
  </key>
  <key>
    <name>O</name>
    <desc>Overhead panel view</desc>
  </key>
  <key>
    <name>Alt+S</name>
    <desc>Toggle superchargers low/high</desc>
  </key>
  <key>
    <name>Ctrl+V</name>
    <desc>Pilot view</desc>
  </key>
  <key>
    <name>Delete</name>
    <desc>Engage/Disengage Prop Reverse</desc>
  </key>
  <key>
    <name>Ctrl+Z</name>
    <desc>Toggle autopilot on/off</desc>
  </key>

  <!-- FDM ops -->

  <text>
Starting the Constellation's engines:

Engage the magnetos for the engines you wish to start by setting the
switches above the pilot seat to "Both". From the engineer's station,
locate the "MJB No. 1" panel to the upper left. Turn on the ship's
battery or ground cart battery. Turn on all generator switches. Below
that panel, find the "MJB No. 2" panel. Turn the "Engine Starter Select"
switch to the engine you want to start. Press "Start" and watch your
gauges for the engine to catch. Repeat for all 4 engines.

________________________Procedures_________________________
Takeoff :
Open cowl flaps 100%.
flaps 60%.
Full throttle, 2900 RPM.
120 KIAS (light load) or 130 KIAS (full load): rotate
165 KIAS: gear up
184 KIAS: flaps up

Climb :
48.0 inhg, 2600 RPM.
Cowl flaps 60%
2000 fpm until 10000 ft.
Engage supercharger high speed above 8500 ft.
1500 fpm until 13000 ft,
1000 fpm above 13000 ft.
Gradually lean mixture to keep BMEP as high as possible.
Watch cylinder head temperature; open cowl flaps if necessary.

Cruise :
223 KIAS at 20000 ft, 218 KIAS at 21000 ft
Close cowl flaps.

Descent :
max pitch, 48.0 inHg or less as necessary.
Gradually enrich mixture to keep BMEP maximized.
Engage supercharger low speed below 9000 ft.

Approach :
184 KIAS: flaps 60%
165 KIAS: gear down
161 KIAS: flaps 66%
154 KIAS: flaps 80%
148 KIAS: flaps 100%

Landing :
maintain 120 kt (landing load);
touch down 110 kt (landing load), 100 kt (empty load).

________________________Emergency_________________________
Put out fire :
At Engineer View:

Mixture  lever for this engine down
Throttle lever for this engine down

Restart after fire :
Magnetos for this engine to both
Mixture max. (or same as others)
Throttle max. (or same as others)
Starter switch to the engine no....
and restart with S or starter button

<!-- Real data -->
________________________ Performance _______________________
Ceiling : 23500 ft
Normal cruise : 280 KTAS (223 KIAS) @ 20000 ft
Range : 3800 nmi

_______________________ Speed limits _______________________
Vne (never exceed) : 294 KIAS until 12500 ft; then - 10 KIAS / 2000 ft
Vno (normal operation): 261 KIAS until 12500 ft, then - 10 KIAS / 2000 ft
Va (maneuvering) : 193 KIAS
Vlo (landing gear operation) : 165 KIAS
Vle (landing gear extension) : 165 KIAS
Vf (flaps):
 take-off   60%: 195 KIAS
 approach   66%: 174 KIAS
 final      80%: 174 KIAS
 landing   100%: 165 KIAS

________________________ Engine limits _____________________
Maximum take-off power: 2900 rpm, 3250 hp
2 minutes at sea level : 56.5 inHg
5 minutes at 7500 ft   : 53.5 inHg

Maximum continuous power: 2600 rpm
sea level: 49.0 inHg, 2700 hp
 5800 ft:  47.0 inHg, 2750 hp
10050 ft:  48.5 inHg, 2400 hp
16400 ft:  47.0 inHg, 2450 hp

Maximum cylinder head temperature: 270 degC, 550 degF

________________________ Weight limits _____________________
See Equipment > Fuel and payload.
The center of gravity must lie within the following limits:

At 137500 lbs: between 671.3 and 685.2 inches aft of the nose
At  90000 lbs: between 660.5 and 685.2 inches aft of the nose
  </text>

</PropertyList>
