<PropertyList>
	<name>Takeoff</name>
	<description>

		This tutorial will teach you how to take-off, and climb at the optimum speed of 185 mph. You will level off at 10000ft to complete the tutorial.
	</description>
	<audio-dir>Aircraft/spitfire/tutorial</audio-dir>
	<timeofday>noon</timeofday>
	<!--<presets>
    <airport-id>KSFO</airport-id>
    <on-ground>1</on-ground>
    <runway>28R</runway>
    <altitude-ft>-9999</altitude-ft>
    <latitude-deg>-9999</latitude-deg>
    <longitude-deg>-9999</longitude-deg>
    <heading-deg>2800</heading-deg>
    <airspeed-kt>0</airspeed-kt>
    <glideslope-deg>0</glideslope-deg>
    <offset-azimuth-deg>0</offset-azimuth-deg>
    <offset-distance-nm>0</offset-distance-nm>
  </presets>-->

	<init>
		<set>
			<property>/sim/current-view/view-number</property>
			<value>0</value>
		</set>
		<set>
			<property>/controls/gear/brake-parking</property>
			<value>1</value>
		</set>
		<set>
			<property>/controls/flight/flaps</property>
			<value>0.0</value>
		</set>
		<set>
			<property>/controls/engines/engine/mag-switch-left/</property>
			<value>1</value>
		</set>
		<set>
			<property>/controls/engines/engine/mag-switch-right/</property>
			<value>1</value>
		</set>
		<set>
			<property>/controls/engines/engine/magnetos</property>
			<value>3</value>
		</set>
		<set>
			<property>/controls/engines/engine/throttle</property>
			<value>0.3</value>
		</set>
		<set>
			<property>/engines/engine/primer</property>
			<value>5</value>
		</set>
		<set>
			<property>/controls/engines/engine/starter</property>
			<value>true</value>
		</set>
		<set>
			<property>controls/engines/engine[0]/propeller-pitch</property>
			<value>1</value>
		</set>
		<set>
			<property>/environment/weather-scenario</property>
			<value>Fair weather</value>
		</set>
		<set>
			<property>/controls/flight/door-position-norm</property>
			<value>0.0</value>
		</set>
		<set>
			<property>controls/engines/engine/cowl-flaps-norm</property>
			<value>1.0</value>
		</set>
	</init>

	<step>
		<message>
			At the start of the take-off roll, you will control the direction of the aircraft using the
			diffential brake steering and rudder. As the aircraft accelerates, you will use the ailerons and elevator
			to control the direction and attitude of the aircraft.
		</message>
		<set>
			<property>/controls/engines/engine/starter</property>
			<value>false</value>
		</set>
		<set>
			<property>/controls/engines/engine/throttle</property>
			<value>0.2</value>
		</set>
	</step>

	<step>
		<message>
			The differential brakes are controlled using the keys ','and '.' .
			The rudder is controlled using 0/Enter on the numeric keypad, or by using the mouse
			in "yoke" mode with the left mouse button held down.
			To switch the mouse to yoke mode, press the right mouse button until it displays as a + sign.
		</message>
	</step>

	<step>
		<message>
			The Spitfire is easier to control using joystick or yoke.
			Almost all the following keyboard instructions can be carried out by means of the mouse, however
			you will probably find the keyboard easier.
		</message>
	</step>

	<step>
		<message>
			TESTING ENGINE AND INSTALLATIONS
		</message>
		<set>
			<property>/controls/engines/engine/starter</property>
			<value>false</value>
		</set>
		<set>
			<property>/controls/engines/engine/throttle</property>
			<value>0.0</value>
		</set>
	</step>

	<step>
		<message>Check Radiator Flap lever is set to Open (fully forward) using H</message>
		<view>
			<heading-offset-deg>11.4</heading-offset-deg>
			<pitch-offset-deg>-39.3</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.5000</x-m>
			<y-m>-0.2058</y-m>
			<z-m>-0.0322</z-m>
			<scale>1.0000</scale>
		</marker>
		<error>
			<message>Check Radiator Flap lever set to Open (fully forward) using H</message>
			<condition>
				<not>
					<equals>
						<property>controls/engines/engine/cowl-flaps-norm</property>
						<value>1</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/engines/engine/cowl-flaps-norm</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check the operation of the RPM lever by setting to min (fully back) using N</message>
		<set>
			<property>/controls/engines/engine/throttle</property>
			<value>0.20</value>
		</set>
		<view>
			<heading-offset-deg>22.5</heading-offset-deg>
			<pitch-offset-deg>-32.9</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.5000</x-m>
			<y-m>-0.2653</y-m>
			<z-m>0.1083</z-m>
			<scale>1.0000</scale>
		</marker>
		<error>
			<message>Check RPM lever is set to min (fully back)</message>
			<condition>
				<not>
					<equals>
						<property>/controls/engines/engine[0]/propeller-pitch</property>
						<value>0</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/controls/engines/engine[0]/propeller-pitch</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<view>
			<heading-offset-deg>22.5</heading-offset-deg>
			<pitch-offset-deg>-32.9</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.5000</x-m>
			<y-m>-0.2653</y-m>
			<z-m>0.1083</z-m>
			<scale>1.0000</scale>
		</marker>
		<message>Check the operation of the RPM lever by setting to max (fully forward) using n</message>
		<error>
			<message>Check RPM lever is set to max (fully forward)</message>
			<condition>
				<not>
					<equals>
						<property>controls/engines/engine[0]/propeller-pitch</property>
						<value>1</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/engines/engine[0]/propeller-pitch</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check the brake pressure is at least 120 psi</message>
		<view>
			<heading-offset-deg>19.2</heading-offset-deg>
			<pitch-offset-deg>-41.0</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>30.0</field-of-view>
		</view>
		<marker>
			<x-m>3.3000</x-m>
			<y-m>-0.2769</y-m>
			<z-m>0.0479</z-m>
			<scale>3.0000</scale>
		</marker>
		<error>
			<message>Check the brake pressure is at least 120 psi</message>
			<condition>
				<less-than-equals>
					<property>engines/engine/rpm</property>
					<value>750</value>
				</less-than-equals>
			</condition>
		</error>
		<condition>
			<greater-than>
				<property>engines/engine/rpm</property>
				<value>750</value>
			</greater-than>
		</condition>
	</step>

	<step>
		<message>Check Pneumatic System by setting Flap lever to DOWN by using ]</message>
		<view>
			<heading-offset-deg>18.0</heading-offset-deg>
			<pitch-offset-deg>-17.3</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.3000</x-m>
			<y-m>-0.1959</y-m>
			<z-m>0.3421</z-m>
			<scale>2.0579</scale>
		</marker>
		<error>
			<message>Check Flap lever set to DOWN using ]</message>
			<condition>
				<not>
					<equals>
						<property>controls/flight/flaps-lever</property>
						<value>1</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/flight/flaps-lever</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check Pneumatic System by setting Flap lever to UP by using [</message>
		<view>
			<heading-offset-deg>18.0</heading-offset-deg>
			<pitch-offset-deg>-17.3</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.3000</x-m>
			<y-m>-0.1959</y-m>
			<z-m>0.3421</z-m>
			<scale>2.0579</scale>
		</marker>
		<error>
			<message>Check Flap lever set to UP using [</message>
			<condition>
				<not>
					<equals>
						<property>controls/flight/flaps-lever</property>
						<value>0</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/flight/flaps-lever</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>


	<step>
		<message>Set the Altimeter to zero (ground level) using the knob</message>
		<view>
			<heading-offset-deg>6.1</heading-offset-deg>
			<pitch-offset-deg>-34.6</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>50.4</field-of-view>
		</view>
		<marker>
			<x-m>3.5000</x-m>
			<y-m>-0.0645</y-m>
			<z-m>0.2463</z-m>
			<scale>0.5</scale>
		</marker>
		<error>
			<message>Set the altimeter to zero (ground level) using the knob</message>
			<condition>
				<or>
					<less-than>
						<property>/instrumentation/altimeter/indicated-altitude-ft</property>
						<value>-2.5</value>
					</less-than>
					<greater-than>
						<property>/instrumentation/altimeter/indicated-altitude-ft</property>
						<value>2.5</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<and>
					<greater-than-equals>
						<property>/instrumentation/altimeter/indicated-altitude-ft</property>
						<value>-2.5</value>
					</greater-than-equals>
					<less-than-equals>
						<property>/instrumentation/altimeter/indicated-altitude-ft</property>
						<value>2.5</value>
					</less-than-equals>
				</and>
			</condition>
		</exit>
	</step>

	<step>
		<message>Set DG to the Magnetic Heading using the knob</message>
		<view>
			<heading-offset-deg>6.1</heading-offset-deg>
			<pitch-offset-deg>-34.6</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>50.4</field-of-view>
		</view>
		<marker>
			<x-m>3.3000</x-m>
			<y-m>0.0000</y-m>
			<z-m>0.0868</z-m>
			<scale>1.0000</scale>
		</marker>
	</step>

	<step>
		<message>Check both fuel cock levers set to ON (fully up)</message>
		<view>
			<heading-offset-deg>357.3</heading-offset-deg>
			<pitch-offset-deg>-42.8</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.3000</x-m>
			<y-m>0.0860</y-m>
			<z-m>-0.0653</z-m>
			<scale>2.0579</scale>
		</marker>
		<error>
			<message>Check both fuel cock levers set to ON (fully up)</message>
			<condition>
				<or>
					<not>
						<equals>
							<property>consumables/fuel/tank[0]/selected</property>
							<value>1</value>
						</equals>
					</not>
					<not>
						<equals>
							<property>consumables/fuel/tank[1]/selected</property>
							<value>1</value>
						</equals>
					</not>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<and>
					<equals>
						<property>consumables/fuel/tank[0]/selected</property>
						<value>1</value>
					</equals>
					<equals>
						<property>consumables/fuel/tank[1]/selected</property>
						<value>1</value>
					</equals>
				</and>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check Fuel Level by pressing the button</message>
		<view>
			<heading-offset-deg>338.5</heading-offset-deg>
			<pitch-offset-deg>-33.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.5000</x-m>
			<y-m>0.1504</y-m>
			<z-m>0.2050</z-m>
			<scale>0.5000</scale>
		</marker>
		<error>
			<message>Check Fuel Level by pressing the button</message>
			<condition>
				<not>
					<equals>
						<property>/controls/switches/fuel-gauge</property>
						<value>0</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/controls/switches/fuel-gauge</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check the hood is locked in the open position using F</message>
		<view>
			<heading-offset-deg>144.9</heading-offset-deg>
			<pitch-offset-deg>9.7</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>4.1000</x-m>
			<y-m>-0.0364</y-m>
			<z-m>0.6124</z-m>
			<scale>1.0000</scale>
		</marker>
		<error>
			<message>Check the hood is locked in the open position using F</message>
			<condition>
				<not>
					<equals>
						<property>/controls/flight/canopy-lever</property>
						<value>0.0</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/controls/flight/canopy-lever</property>
					<value>0.00</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check the door is locked in the "half cock" open position using D</message>
		<set>
			<property>/controls/engines/engine/throttle</property>
			<value>0.00</value>
		</set>
		<view>
			<heading-offset-deg>80.8</heading-offset-deg>
			<pitch-offset-deg>-53.1</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.8000</x-m>
			<y-m>-0.3050</y-m>
			<z-m>0.2967</z-m>
			<scale>1.0000</scale>
		</marker>
		<error>
			<message>Check the door is locked in the "half cock" open position using D</message>
			<condition>
				<not>
					<equals>
						<property>/controls/flight/door-position-norm</property>
						<value>0.015</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/controls/flight/door-position-norm</property>
					<value>0.015</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Pick the right chock to remove it</message>
		<set>
			<property>/controls/engines/engine/throttle</property>
			<value>0.00</value>
		</set>
		<set>
			<property>/sim/current-view/view-number</property>
			<value>8</value>
		</set>
		<view>
			<heading-offset-deg>180.0</heading-offset-deg>
			<pitch-offset-deg>0.0</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.1</y-offset-m>
			<z-offset-m>-10.0</z-offset-m>
			<field-of-view>60.0</field-of-view>
		</view>
		<marker>
			<x-m>1.8000</x-m>
			<y-m>0.9380</y-m>
			<z-m>-1.8884</z-m>
			<scale>10.0</scale>
		</marker>
		<error>
			<message>Pick the right chock to remove it</message>
			<condition>
				<equals>
					<property>controls/gear/chock-right</property>
					<value>1</value>
				</equals>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/gear/chock-right</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Pick the left chock to remove it</message>
		<set>
			<property>/controls/engines/engine/throttle</property>
			<value>0.00</value>
		</set>
		<marker>
			<x-m>1.6000</x-m>
			<y-m>-0.3000</y-m>
			<z-m>-1.9000</z-m>
			<scale>10.0000</scale>
		</marker>
		<error>
			<message>Pick the left chock to remove it</message>
			<condition>
				<equals>
					<property>controls/gear/chock-left</property>
					<value>1</value>
				</equals>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/gear/chock-left</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>FINAL PREPARATIONS FOR TAKEOFF - DRILL OF VITAL ACTIONS</message>
		<set>
			<property>/sim/current-view/view-number</property>
			<value>0</value>
		</set>
		<view>
			<heading-offset-deg>0.0</heading-offset-deg>
			<pitch-offset-deg>-9.5</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
	</step>

	<step>
		<message>Some of these may have already been done, but must be checked before every takeoff.</message>
	</step>

	<step>
		<message>Aide Memoire: TMP and Flaps.</message>
	</step>

	<step>
		<message>Set Elevator Trim tab to 1 division Nose Down using Home</message>
		<view>
			<heading-offset-deg>18.2</heading-offset-deg>
			<pitch-offset-deg>-34.1</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>34.2</field-of-view>
		</view>
		<marker>
			<x-m>3.3000</x-m>
			<y-m>-0.1893</y-m>
			<z-m>0.1066</z-m>
			<scale>1.4</scale>
		</marker>
		<error>
			<message>Set Elevator Trim tab to 1 division Nose Down</message>
			<condition>
				<or>
					<less-than>
						<property>/controls/flight/elevator-trim</property>
						<value>0.055</value>
					</less-than>
					<greater-than>
						<property>/controls/flight/elevator-trim</property>
						<value>0.075</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<greater-than-equals>
					<property>/controls/flight/elevator-trim</property>
					<value>0.055</value>
				</greater-than-equals>
				<less-than-equals>
					<property>/controls/flight/elevator-trim</property>
					<value>0.075</value>
				</less-than-equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check Mixture lever is set to RICH (fully back) using m</message>
		<view>
			<heading-offset-deg>39.8</heading-offset-deg>
			<pitch-offset-deg>-43.4</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.55</x-m>
			<y-m>-0.3744</y-m>
			<z-m>0.0405</z-m>
			<scale>1.0</scale>
		</marker>
		<error>
			<message>Check Mixture lever is set to RICH (fully back)</message>
			<condition>
				<equals>
					<property>controls/engines/engine[0]/mixture-lever</property>
					<value>0</value>
				</equals>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/engines/engine[0]/mixture-lever</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check RPM lever is set to MAX (fully forward) using n</message>
		<set>
			<property>/sim/current-view/view-number</property>
			<value>0</value>
		</set>
		<view>
			<heading-offset-deg>22.5</heading-offset-deg>
			<pitch-offset-deg>-32.9</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.5000</x-m>
			<y-m>-0.2653</y-m>
			<z-m>0.1083</z-m>
			<scale>1.0000</scale>
		</marker>
		<error>
			<message>Check RPM lever is set to MAX (fully forward)</message>
			<condition>
				<not>
					<equals>
						<property>controls/engines/engine[0]/propeller-pitch</property>
						<value>1</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/engines/engine[0]/propeller-pitch</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check Flap lever set to UP using [</message>
		<view>
			<heading-offset-deg>18.0</heading-offset-deg>
			<pitch-offset-deg>-17.3</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.3000</x-m>
			<y-m>-0.1959</y-m>
			<z-m>0.3421</z-m>
			<scale>2.0579</scale>
		</marker>
		<error>
			<message>Check Flap lever set to UP using [</message>
			<condition>
				<not>
					<equals>
						<property>controls/flight/flaps-lever</property>
						<value>0</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/flight/flaps-lever</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Check Radiator Flap lever set to Open using H</message>
		<view>
			<heading-offset-deg>25.7</heading-offset-deg>
			<pitch-offset-deg>-50.6</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>
		<marker>
			<x-m>3.6000</x-m>
			<y-m>-0.2157</y-m>
			<z-m>0.0066</z-m>
			<scale>1.5289</scale>
		</marker>
		<error>
			<message>Check Radiator Flap lever set to Open (fully forward)using H</message>
			<condition>
				<not>
					<equals>
						<property>controls/engines/engine/cowl-flaps-norm</property>
						<value>1</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>controls/engines/engine/cowl-flaps-norm</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			TAKEOFF
		</message>
		<view>
			<heading-offset-deg>0.0</heading-offset-deg>
			<pitch-offset-deg>-9.5</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.5</y-offset-m>
			<z-offset-m>3.9</z-offset-m>
			<field-of-view>55.0</field-of-view>
		</view>

		<message>
			The takeoff run is only about 150 yards, and the time is less than 9 seconds.
		</message>
	</step>

	<step>
		<message>
			Release the parking brake using Shift B
		</message>
		<error>
			<message>Release the parking brake using Shift B !</message>
			<condition>
				<or>
				<greater-than>
					<property>/systems/pneumatic/outputs/brake</property>
					<value>0</value>
				</greater-than>
				<greater-than>
					<property>/systems/pneumatic/outputs/brake[1]</property>
					<value>0</value>
				</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/systems/pneumatic/outputs/brake</property>
					<value>0</value>
				</equals>
				<equals>
					<property>/systems/pneumatic/outputs/brake[1]</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Smoothly apply full power using PgUp, controlling the direction using the diffential brakes
			and rudder.
		</message>
		<error>
			<message>RELEASE PARKING BRAKE using Shift B</message>
			<condition>
				<and>
				<greater-than>
					<property>/systems/pneumatic/outputs/brake</property>
					<value>0</value>
				</greater-than>
					<greater-than>
					<property>/systems/pneumatic/outputs/brake[1]</property>
					<value>0</value>
				</greater-than>
				</and>
			</condition>
		</error>
		<error>
			<message>Incease throttle to take-off power. Boost should not exceed 9.0 psi</message>
			<condition>
				<less-than>
					<property>/controls/engines/engine/throttle</property>
					<value>0.5</value>
				</less-than>
			</condition>
		</error>
		<exit>
			<condition>
				<greater-than>
					<property>/velocities/airspeed-kt</property>
					<value>5.0</value>
				</greater-than>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Watch out for the swing to the left as the tail comes up. Correct quickly using coarse right rudder.
			Stay on the center-line of the runway using the rudder. Steer using the mouse with the left button held down, or using 0/Enter on the numeric keypad
		</message>
		<exit>
			<condition>
				<greater-than>
					<property>/velocities/airspeed-kt</property>
					<value>45.0</value>
				</greater-than>
			</condition>
		</exit>
	</step>

	<step>
		<message>Let the aircraft lift off at about 85 mph and climb straight out on runway heading.</message>
		<error>
			<message>Gently raise the nose, by pressing the down key on the keypad, or moving the mouse back slightly.</message>
			<condition>
				<equals>
					<property>/gear/gear[0]/wow</property>
					<value>1</value>
				</equals>
			</condition>
		</error>
		<exit>
			<condition>
				<not>
					<property>/gear/gear[0]/wow</property>
					<value>1</value>
				</not>
			</condition>
		</exit>
	</step>

	<step>
		<message>ACTIONS AFTER TAKEOFF</message>
	</step>

	<step>
		<message>As soon as the aircraft is FINALLY off the ground, raise the undercarriage using g.</message>
		<error>
			<condition>
				<equals>
					<property>/gear/gear/position-norm</property>
					<value>1</value>
				</equals>
			</condition>
		</error>
		<exit>
			<condition>
				<not>
					<equals>
						<property>/gear/gear/position-norm</property>
						<value>1</value>
					</equals>
				</not>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Keep the nose down until 140 mph is attained then raise the nose to start climbing at
			185 mph
		</message>
		<error>
			<message>
				Keep the nose down. Do not start climbing.
			</message>
			<condition>
				<less-than>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>121.5</value>
				</less-than>
			</condition>
		</error>
		<exit>
			<message>
				Raise the nose. Climb at 185 mph
			</message>
			<condition>
				<greater-than-equals>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>121.5</value>
				</greater-than-equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Adjust the RPM to 2850 rpm using N/n. Raise/Lower the nose to maintain 185mph
		</message>
		<error>
			<message>
				Lower the nose.
			</message>
			<condition>
				<less-than-equals>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>145</value>
				</less-than-equals>
			</condition>
		</error>
		<error>
			<message>
				Lower the nose slightly.
			</message>
			<condition>
				<less-than>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>155</value>
				</less-than>
			</condition>
		</error>
		<error>
			<message>
				Raise the nose slightly.
			</message>
			<condition>
				<greater-than-than>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>165</value>
				</greater-than-than>
			</condition>
		</error>
		<error>
			<message>
				Raise the nose.
			</message>
			<condition>
				<greater-than-equals>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>175</value>
				</greater-than-equals>
			</condition>
		</error>
		<error>
			<message>
				Decrease rpm using N.
			</message>
			<condition>
				<greater-than-equals>
					<property>engines/engine/rpm</property>
					<value>2900</value>
				</greater-than-equals>
			</condition>
		</error>
		<error>
			<message>
				Increase rpm using n.
			</message>
			<condition>
				<less-than-equals>
					<property>engines/engine/rpm</property>
					<value>2800</value>
				</less-than-equals>
			</condition>
		</error>
		<error>
			<message>
				Close the door, close the hood, shut the radiator flap using d,f, and h
			</message>
			<condition>
				<or>
					<not>
						<equals>
							<property>/controls/flight/door-position-norm</property>
							<value>0</value>
						</equals>
					</not>
					<not>
						<equals>
							<property>/controls/engines/engine/cowl-flaps-norm</property>
							<value>0</value>
						</equals>
					</not>
					<not>
						<equals>
							<property>/gear/canopy/position-norm</property>
							<value>0</value>
						</equals>
					</not>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<and>
					<equals>
						<property>/controls/flight/door-position-norm</property>
						<value>0</value>
					</equals>
					<equals>
						<property>/controls/engines/engine/cowl-flaps-norm</property>
						<value>0</value>
					</equals>
					<equals>
						<property>/gear/canopy/position-norm</property>
						<value>0</value>
					</equals>
				</and>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Continue to climb. You can adjust pitch and roll with the elevator and rudder trims using Home/End 
			and shift, or shift . (Yes, rudder trim affects roll).
		</message>
		<error>
			<message>
				Passing 4000 ft adjust the Oxygen Regulator to 15000 ft using the key.
			</message>
			<condition>
				<and>
				<less-than>
					<property>/controls/oxygen/altitude-norm</property>
					<value>0.37</value>
				</less-than>
					<greater-than>
						<property>instrumentation/altimeter/indicated-altitude-ft</property>
						<value>4000</value>
					</greater-than>
				</and>
			</condition>
		</error>
		<error>
			<message>
				Lower the nose.
			</message>
			<condition>
				<less-than-equals>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>145</value>
				</less-than-equals>
			</condition>
		</error>
		<error>
			<message>
				Lower the nose slightly.
			</message>
			<condition>
				<less-than>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>155</value>
				</less-than>
			</condition>
		</error>
		<error>
			<message>
				Raise the nose slightly.
			</message>
			<condition>
				<greater-than-than>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>165</value>
				</greater-than-than>
			</condition>
		</error>
		<error>
			<message>
				Raise the nose.
			</message>
			<condition>
				<greater-than-equals>
					<property>instrumentation/airspeed-indicator/indicated-speed-kt</property>
					<value>175</value>
				</greater-than-equals>
			</condition>
		</error>
		<error>
			<message>
				Decrease rpm using N.
			</message>
			<condition>
				<greater-than-equals>
					<property>engines/engine/rpm</property>
					<value>2900</value>
				</greater-than-equals>
			</condition>
		</error>
		<error>
			<message>
				Increase rpm using n.
			</message>
			<condition>
				<less-than-equals>
					<property>engines/engine/rpm</property>
					<value>2800</value>
				</less-than-equals>
			</condition>
		</error>
		<exit>
			<condition>
				<greater-than-equals>
					<property>instrumentation/altimeter/indicated-altitude-ft</property>
					<value>10000</value>
				</greater-than-equals>
			</condition>
		</exit>
	</step>

	<end>
		<message>Congratulations, you've successfully taken off. Now try landing!</message>
	</end>
</PropertyList>
