AKMCS                   Active learning reliability method combining
                        Kriging and Monte Carlo Simulation
BMP                     Bayesian Moving Particles
ComputeDistributionParameter
                        Compute internal parameters and moments for
                        univariate distribution functions
FORM                    First-order reliability method
FORMv0                  FORM method (old version)
IRW                     Increasing Randow Walk
LSVM                    Linear Support Vector Machine under
                        monotonicity constraints
MP                      Moving Particles
MetaIS                  Metamodel based Impotance Sampling
MetropolisHastings      The modified Metropolis-Hastings algorithm
ModifCorrMatrix         Modification of a correlation matrix to use in
                        UtoX
MonotonicQuantileEstimation
                        Quantile estimation under monotonicity
                        constraints
MonteCarlo              Crude Monte Carlo method
S2MART                  Subset by Support vector Margin Algorithm for
                        Reliability esTimation
SMART                   Support-vector Margin Algoritm for Reliability
                        esTimation
SubsetSimulation        Subset Simulation Monte Carlo
UtoX                    Iso-probabilistic transformation from U space
                        to X space
WilksFormula            Sample size by Wilks formula
XtoU                    From X to standard space
cantilever              A function calculating the deviation of a
                        cantilever beam.
estimateSUR             EstimateSUR
generateK               Generate Standard Gaussian samples with a
                        Gaussian transiiton kernel
kiureghian              A limit-state-function defined by Der
                        Kiureghian
mistral-package         Methods In Structural Reliability Analysis
modelLSVM               Estimation of the parameters of the LSVM
ok                      Class of Ordinary Kriging
oscillator_d6           A limit-state-function defined with a
                        non-linear oscillator in dimension 6.
plotLSVM                plot of LSVM
precomputeUpdateData    precomputeUpdateData
quantileWilks           Computing quantiles with the Wilks formula
rackwitz                A limit-state-function defined by Rackwitz
testConvexity           Test the convexity of set of data
twodof                  A limit-state-function defined with a two
                        degrees of freedom damped oscillator
updateLSVM              Update LSVM classifier
updateSd                UpdateSd
updateSd.old            UpdateSd.old
waarts                  A limit-state-function defined by Waarts
